# lpstate Struct Reference

`#include <lpstate.h>`

## Data Fields
uint16_t | listen_period
uint16_t | chirp_period

## Detailed Description

Arch Rock Low Power Protocol Parameter Settings.

## Field Documentation

uint16_t lpstate::listen_period

Specify the radio wake up period in milliseconds Recommended default is 64ms.

uint16_t lpstate::chirp_period

Specify the radio chirp period in millisconds. Recommended default is to keep this the same as listen period.

The documentation for this struct was generated from the following file:

- lpstate.h